
**Steps for Implementing Star Topology**


**Step 1: Ta**ke a switch and linked it to six end devices.

****

**Step 2:** Link every device with the switch.

**Step 3:** Provide the IP address to each device.

**Step 4:**Transfer message from one device to another and check the Table for Validation.

****

Now to check whether the connections are correct or not, try to ping any device

ping 192.168.1.4

Note: If the connections are correct then you will receive the response.

